TOPSPIN indoor
Kg 96   EN 14468-1   CE   COMPACT SYSTEM
Cod. TOPSPIN-IC • antracite | charcoal   EAN: 8029975920429
152,5 cm; 142,2 cm; 159 cm; 76 cm; 104 cm; 163,5 cm
152,5 cm; 159 cm; 104 cm; 45 cm
Tavolo per interno, pieghevole, coniuga praticità, robustezza e qualità. Piano di gioco e telaio, entrambi in elegante finitura antracite, valorizzano un tavolo realizzato nelle dimensioni regolamentari da torneo (274 × 152,5 x 76 cm), per un'esperienza di gioco autentica e coinvolgente. Solido e affidabile, è progettato per garantire prestazioni elevate anche in caso di utilizzo intensivo, risultando la scelta ideale per scuole, comunità, oratori e altre strutture ricreative.
Il piano di gioco è realizzato in fibra di legno ad alta densità (HDF) con rivestimento melaminico da 18 mm di spessore, caratterizzato da finitura antiriflesso e linee di gioco bianche indelebili.
Il tavolo è fornito di rete e tendirete approvata ITTF, da rimuovere per richiudere il tavolo. Possibilità di regolare la tensione della rete.
Il telaio e le gambe sono realizzati in tubolare metallico da 40x40 mm con verniciatura a polvere e rinforzati da traverse e barre di collegamento orizzontali, per garantire un'eccellente stabilità e una straordinaria robustezza anche in caso di utilizzo intensivo.
I piedini regolabili assicurano un perfetto livellamento del tavolo, contribuendo a migliorare la stabilità della struttura e la regolarità del rimbalzo della pallina.
Il sistema di sicurezza integrato, con meccanismo di sblocco ergonomico, consente un'apertura agevole e assicura la massima sicurezza durante le operazioni di apertura, chiusura e movimentazione del tavolo.
Gli spostamenti risultano semplici e sicuri grazie alle otto ruote da 75 mm di diametro, tutte piroettanti a 360° e dotate di freno.
Garanzia sui difetti di fabbricazione: 2 anni.

A foldable indoor table tennis table, combining practicality, stability and quality. The elegant anthracite-finished playing surface and frame, together with official tournament dimensions (274×152.5×76 cm), deliver an authentic and engaging playing experience. Sturdy and reliable, it is designed to ensure outstanding performance even under intensive use, making it the ideal choice for schools, community centres, youth clubs and other recreational facilities.
The 18 mm thick playing surface is made of high density fibreboard (HFD) with a melamine coating, featuring an anti-glare finish and permanently printed white playing lines.
The table is supplied with an ITTF-approved net and post set, which must be removed before folding the table. The net tension can be easily adjusted.
The frame and legs are constructed from 40x40 mm powder-coated steel tubing and reinforced with cross braces and horizontal connecting bars, ensuring exceptional stability and outstanding strength even under intensive use.
The adjustable leg levellers ensure the table is perfectly level, enhancing the stability of the structure and providing a more consistent ball bounce.
The integrated safety system, featuring an ergonomic release mechanism, allows smooth opening while ensuring maximum safety during opening, folding and transportation.
The table can be moved easily and safely thanks to eight 75 mm diameter swivel wheels with 360° rotation, all equipped with brakes.
Warranty against manufacturing defects: 2 years.
